Assembly Instructions: Trolley MS-3205A (Large)
Contents:
4 x wheels
3 x trays
8 x poles
1 x handle
12 x skinny pole small
6 x skinny pole large
4 x connectors
2 x rectangular containers
2 x yellow buckets with lids
1 x side basket
1 x bucket with handle

Step 1:
Remove contents from box and layout all pieces
Step 2: 
Start by adding the 4 sets of wheels to the bottom of the base you do this by pushing the wheel through the hole and twisting the thick connecting poles to attach by the wheel till in tight. 
Step 3: 
Gather all small connections, add the skinny larges poles to the holes provided on small connections. Make sure side without poles is facing the base with the slight slant as picture provided. This to make sure your still able to access items on tray 
Step 4 :
Repeat step 3 & 2 except the wheels, as shown above for the 3rd tray  take the grey inner

Step 5 :  
Take the handle and place in the holes provided on the top stay 
Place the last tray with built in draws on top. Attach the side container & 2 rectangle containers to the given side of the trolly,
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